### - m -

- macAddress : CSL_CPSW_3GF_ALE_MCASTADDR_ENTRY , CSL_CPSW_3GF_ALE_VLANMCASTADDR_ENTRY , CSL_CPSW_3GF_ALE_VLANUNICASTADDR_ENTRY , CSL_CPSW_3GF_ALE_UNICASTADDR_ENTRY
- major_version : CSL_SGMII_VERSION
- majorVer : CSL_CPSW_3GF_ALE_VERSION , CSL_CPSW_3GFSS_VERSION , CSL_CPTS_VERSION , CSL_CPGMAC_SL_VERSION , CSL_CPSW_3GF_VERSION
- mask : CSL_IDMA_IDMA0CONFIG
- maxWait : CSL_BWMNGMT_CPUARB_SETUP
- mcastFwdState : CSL_CPSW_3GF_ALE_MCASTADDR_ENTRY , CSL_CPSW_3GF_ALE_VLANMCASTADDR_ENTRY
- mcastLimit : CSL_CPSW_3GF_ALE_PORTCONTROL
- minor_version : CSL_SGMII_VERSION
- minorVer : CSL_CPTS_VERSION , CSL_CPGMAC_SL_VERSION , CSL_CPSW_3GFSS_VERSION , CSL_CPSW_3GF_ALE_VERSION , CSL_CPSW_3GF_VERSION
- missed : CSL_Edma3ChannelErr
- modId : CSL_MDIO_VERSION
- msgType : CSL_CPTS_EVENTINFO

Copyright 2012, Texas Instruments Incorporated