# csl_idma.h File Reference

IDMA CSL Implementation on DSP side. More...

`#include <ti/csl/soc.h>`
`#include <ti/csl/csl.h>`
`#include <ti/csl/cslr_cgem.h>`

## Data Structures
struct | CSL_IDMA_IDMA1CONFIG
| This structure holds the information required to initiate a iDMA Channel 1 Block Fill/Transfer request in the GEM. More...
struct | CSL_IDMA_IDMA0CONFIG
| This structure holds the information required to initiate a iDMA Channel 0 Configuration(CFG) space Transfer request from the GEM. More...
struct | CSL_IDMA_STATUS
| This structure holds the information required to interpret the IDMA Channel 0/1 Transfer Status. More...
## Defines
#define | hIdma ((CSL_CgemRegs *) CSL_CGEM0_5_REG_BASE_ADDRESS_REGS)
## Enumerations
enum | IDMA_priSet { IDMA_PRI_0 = 0, IDMA_PRI_1, IDMA_PRI_2, IDMA_PRI_3, IDMA_PRI_4, IDMA_PRI_5, IDMA_PRI_6, IDMA_PRI_7, IDMA_PRI_NULL = -1 }

## Detailed Description

IDMA CSL Implementation on DSP side.

  ============================================================================
  (C) Copyright 2008, 2009, Texas Instruments, Inc.
  Use of this software is controlled by the terms and conditions found
  in the license agreement under which this software has been supplied. ===========================================================================

Copyright 2012, Texas Instruments Incorporated