# CSL_CPSW_3GF_ALE_UNICASTADDR_ENTRY Struct Reference
[CPSW_3GF Data Structures]

Holds the ALE Unicast Address Table entry configuration. More...

`#include <csl_cpsw_3gf.h>`

## Data Fields
Uint8 | macAddress [6]
CSL_CPSW_3GF_ALE_UCASTTYPE | ucastType
Uint32 | secureEnable
Uint32 | blockEnable
Uint32 | portNumber

## Detailed Description

Holds the ALE Unicast Address Table entry configuration.

## Field Documentation

Uint32 CSL_CPSW_3GF_ALE_UNICASTADDR_ENTRY::blockEnable

Block bit enable?

Uint8 CSL_CPSW_3GF_ALE_UNICASTADDR_ENTRY::macAddress[6]

Unicast address

Uint32 CSL_CPSW_3GF_ALE_UNICASTADDR_ENTRY::portNumber

Port Number to forward matching packets to.

Uint32 CSL_CPSW_3GF_ALE_UNICASTADDR_ENTRY::secureEnable

Secure bit enable?

CSL_CPSW_3GF_ALE_UCASTTYPE CSL_CPSW_3GF_ALE_UNICASTADDR_ENTRY::ucastType

Unicast type

The documentation for this struct was generated from the following file:

- csl_cpsw_3gf.h

Copyright 2012, Texas Instruments Incorporated