# CSL_Edma3ActivityStat Struct Reference
[EDMA3 Data Structures]

Edma Channel Controller Activity Status. More...

`#include <csl_edma3.h>`

## Data Fields
Uint16 | outstandingTcc
CSL_BitMask16 | queActive
Bool | active
Bool | qevtActive
Bool | evtActive
Bool | trActive

## Detailed Description

Edma Channel Controller Activity Status.

An object of this type is allocated by the user and its address is passed as a parameter to the CSL_edma3GetActivityStatus() /CSL_edma3GetHwStatus().

## Field Documentation

Bool CSL_Edma3ActivityStat::active

Indicates if the Channel Controller is active at all

Bool CSL_Edma3ActivityStat::evtActive

Indicates whether any EDMA events are active

Uint16 CSL_Edma3ActivityStat::outstandingTcc

Number of outstanding completion requests

Bool CSL_Edma3ActivityStat::qevtActive

Indicates whether any QDMA events are active

CSL_BitMask16 CSL_Edma3ActivityStat::queActive

BitMask of the que active in the Channel Controller

Bool CSL_Edma3ActivityStat::trActive

Indicates whether the TR processing/submission logic is active

The documentation for this struct was generated from the following file:

- csl_edma3.h

Copyright 2012, Texas Instruments Incorporated