# CSL_CPSW_3GF_ALE_PORTCONTROL Struct Reference
[CPSW_3GF Data Structures]

Holds the ALE Port control register info. More...

`#include <csl_cpsw_3gf.h>`

## Data Fields
CSL_CPSW_3GF_ALE_PORTSTATE | portState
Uint32 | dropUntaggedEnable
Uint32 | vidIngressCheckEnable
Uint32 | noLearnModeEnable
Uint32 | mcastLimit
Uint32 | bcastLimit

## Detailed Description

Holds the ALE Port control register info.

## Field Documentation

Uint32 CSL_CPSW_3GF_ALE_PORTCONTROL::bcastLimit

Broadcast packet rate limit

Uint32 CSL_CPSW_3GF_ALE_PORTCONTROL::dropUntaggedEnable

Drop non-VLAN tagged ingress packets?

Uint32 CSL_CPSW_3GF_ALE_PORTCONTROL::mcastLimit

Multicast packet rate limit

Uint32 CSL_CPSW_3GF_ALE_PORTCONTROL::noLearnModeEnable

No learn mode enable

CSL_CPSW_3GF_ALE_PORTSTATE CSL_CPSW_3GF_ALE_PORTCONTROL::portState

Port state

Uint32 CSL_CPSW_3GF_ALE_PORTCONTROL::vidIngressCheckEnable

VLAN ID Ingress check enable

The documentation for this struct was generated from the following file:

- csl_cpsw_3gf.h

Copyright 2012, Texas Instruments Incorporated