# CSL_CPTS_EVENTINFO Struct Reference
[CPTS Data Structures]

Holds Time sync event info contents. More...

`#include <csl_cpts.h>`

## Data Fields
Uint32 | timeStamp
Uint32 | seqId
Uint32 | msgType
Uint32 | eventType
Uint32 | portNo

## Detailed Description

Holds Time sync event info contents.

## Field Documentation

Uint32 CSL_CPTS_EVENTINFO::eventType

Event Type read from CPTS EVENT_HIGH register

Uint32 CSL_CPTS_EVENTINFO::msgType

Message Type read from CPTS EVENT_HIGH register

Uint32 CSL_CPTS_EVENTINFO::portNo

Port number read from CPTS EVENT_HIGH register

Uint32 CSL_CPTS_EVENTINFO::seqId

Sequence Id read from CPTS EVENT_HIGH register

Uint32 CSL_CPTS_EVENTINFO::timeStamp

Time stamp read from the CPTS EVENT_LOW register

The documentation for this struct was generated from the following file:

- csl_cpts.h

Copyright 2012, Texas Instruments Incorporated