# CSL_XMC_XPFADDR Struct Reference
[XMC Data Structures]

This is the definition of CSL_XMC_XPFADDR. More...

`#include <csl_xmc.h>`

## Data Fields
Uint32 | addr
Uint32 | dir
Uint32 | dph
Uint32 | dvh
Uint32 | avh
Uint32 | dpl
Uint32 | dvl
Uint32 | avl

## Detailed Description

This is the definition of CSL_XMC_XPFADDR.

## Field Documentation

Uint32 CSL_XMC_XPFADDR::addr

Stream address (128-bit aligned)

Uint32 CSL_XMC_XPFADDR::avh

Address valid for upper half

Uint32 CSL_XMC_XPFADDR::avl

Address valid for lower half

Uint32 CSL_XMC_XPFADDR::dir

Sign bit of stream direction (0=fwd, 1=rev)

Uint32 CSL_XMC_XPFADDR::dph

Data pending for upper ("high") half

Uint32 CSL_XMC_XPFADDR::dpl

Data pending for lower half

Uint32 CSL_XMC_XPFADDR::dvh

Data valid for upper half

Uint32 CSL_XMC_XPFADDR::dvl

Data valid for lower half

The documentation for this struct was generated from the following file:

- csl_xmc.h

Copyright 2012, Texas Instruments Incorporated