# Interrupt selection
[TSIP Enumerated Data Types]

TSIP Interrupt selection. More...

## Enumerations
enum | CSL_TsipInt { CSL_TSIP_INT_ACK = 0, CSL_TSIP_INT_DLY = 1, CSL_TSIP_INT_ACKORDLY = 2, CSL_TSIP_INT_ACKNDLY = 3 }

## Detailed Description

TSIP Interrupt selection.

Use this symbol to set the interrupt selection time This symbol could be used for both RCV and XMT

## Enumeration Type Documentation

enum CSL_TsipInt

Enumerator:

  CSL_TSIP_INT_ACK | Interrupt on Acknowledgement
  CSL_TSIP_INT_DLY | Interrupt on Delay
  CSL_TSIP_INT_ACKORDLY | Interrupt on either Acknowledgement or Delay
  CSL_TSIP_INT_ACKNDLY | Interrupt on both Acknowledgement and Delay

Copyright 2012, Texas Instruments Incorporated