# csl_bootcfgAux.h File Reference

This is the Boot Configuration Auxilary Header File which exposes the various CSL Functional Layer API's to configure the BOOTCFG Module. More...

`#include <ti/csl/csl_bootcfg.h>`

## Functions
CSL_IDEF_INLINE void | CSL_BootCfgGetRevisionInfo (Uint32 *info)
CSL_IDEF_INLINE void | CSL_BootCfgGetDeviceId (Uint32 *id)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsLittleEndian (void)
CSL_IDEF_INLINE Uint16 | CSL_BootCfgGetBootMode (void)
CSL_IDEF_INLINE void | CSL_BootCfgSetBootMode (Uint16 bootMode)
CSL_IDEF_INLINE Uint8 | CSL_BootCfgGetPCIEMode (void)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsPCIEEnabled (void)
CSL_IDEF_INLINE Uint8 | CSL_BootCfgGetPARefClockSelect (void)
CSL_IDEF_INLINE void | CSL_BootCfgUnlockKicker (void)
CSL_IDEF_INLINE void | CSL_BootCfgLockKicker (void)
CSL_IDEF_INLINE Uint32 | CSL_BootCfgGetDSPBootAddress (Uint8 coreIdx)
CSL_IDEF_INLINE void | CSL_BootCfgSetDSPBootAddress (Uint8 coreIdx, Uint32 bootAddress)
CSL_IDEF_INLINE void | CSL_BootCfgGetMacIdentifier (Uint32 *macId1, Uint32 *macId2)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsBootComplete (Uint8 coreIdx)
CSL_IDEF_INLINE void | CSL_BootCfgSetBootComplete (Uint8 coreIdx)
CSL_IDEF_INLINE Uint32 | CSL_BootCfgGetBootProgress (void)
CSL_IDEF_INLINE void | CSL_BootCfgSetBootProgress (Uint32 bootProgress)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsCoreLocalReset (Uint8 coreIdx)
CSL_IDEF_INLINE void | CSL_BootCfgClearLocalReset (Uint8 coreIdx)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsGlobalReset (void)
CSL_IDEF_INLINE void | CSL_BootCfgClearGlobalReset (void)
CSL_IDEF_INLINE void | CSL_BootCfgGetNMILocalResetStatus (Uint8 coreIdx, Uint8 *nmiStatus, Uint8 *localStatus)
CSL_IDEF_INLINE void | CSL_BootCfgClearNMILocalResetStatus (Uint8 coreIdx, Uint8 nmiStatus, Uint8 localStatus)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsSysClockEnabled (void)
CSL_IDEF_INLINE void | CSL_BootCfgEnableSysClock (void)
CSL_IDEF_INLINE void | CSL_BootCfgDisableSysClock (void)
CSL_IDEF_INLINE void | CSL_BootCfgGetPowerStatus (Uint8 *standby, Uint8 *hibernation, Uint8 *hibernationMode, Uint32 *generalPurpose)
CSL_IDEF_INLINE void | CSL_BootCfgSetPowerStatus (Uint8 standby, Uint8 hibernation, Uint8 hibernationMode, Uint32 generalPurpose)
CSL_IDEF_INLINE void | CSL_BootCfgGetSRIOSERDESStatus (Uint32 *srioSERDESStatus)
CSL_IDEF_INLINE void | CSL_BootCfgGetSGMIISERDESStatus (Uint32 *sgmiiSERDESStatus)
CSL_IDEF_INLINE void | CSL_BootCfgGetPCIESERDESStatus (Uint32 *pcieSERDESStatus)
CSL_IDEF_INLINE void | CSL_BootCfgGetVUSRSERDESStatus (Uint32 *vusrSERDESStatus)
CSL_IDEF_INLINE void | CSL_BootCfgGenerateNMIEvent (Uint8 coreNum)
CSL_IDEF_INLINE void | CSL_BootCfgGenerateInterDSPInterrupt (Uint8 coreNum, Uint32 sourceId)
CSL_IDEF_INLINE void | CSL_BootCfgGenerateExternalHostInterrupt (Uint32 sourceId)
CSL_IDEF_INLINE void | CSL_BootCfgGetInterDSPInterruptStatus (Uint8 coreNum, Uint32 *intStatus)
CSL_IDEF_INLINE void | CSL_BootCfgClearInterDSPInterruptStatus (Uint8 coreNum, Uint32 intStatus)
CSL_IDEF_INLINE void | CSL_BootCfgGetExternalHostInterruptStatus (Uint32 *intStatus)
CSL_IDEF_INLINE void | CSL_BootCfgClearExternalHostInterruptStatus (Uint32 intStatus)
CSL_IDEF_INLINE Uint16 | CSL_BootCfgGetTimerInputSelection (void)
CSL_IDEF_INLINE void | CSL_BootCfgSetTimerInputSelection (Uint16 timerInput)
CSL_IDEF_INLINE void | CSL_BootCfgGetTimerOutputSelection (Uint8 *timerOutputSel0, Uint8 *timerOutputSel1)
CSL_IDEF_INLINE void | CSL_BootCfgSetTimerOutputSelection (Uint8 timerOutputSel0, Uint8 timerOutputSel1)
CSL_IDEF_INLINE void | CSL_BootCfgGetResetMuxLockStatus (Uint8 coreIdx, Uint8 *lockStatus)
CSL_IDEF_INLINE void | CSL_BootCfgSetResetMuxLockStatus (Uint8 coreIdx, Uint8 lockStatus)
CSL_IDEF_INLINE void | CSL_BootCfgGetResetMuxOutputMode (Uint8 coreIdx, Uint8 *outputMode)
CSL_IDEF_INLINE void | CSL_BootCfgSetResetMuxOutputMode (Uint8 coreIdx, Uint8 outputMode)
CSL_IDEF_INLINE void | CSL_BootCfgGetResetMuxDelay (Uint8 coreIdx, Uint8 *delay)
CSL_IDEF_INLINE void | CSL_BootCfgSetResetMuxDelay (Uint8 coreIdx, Uint8 delay)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsResetMuxEventDetected (Uint8 coreIdx)
CSL_IDEF_INLINE void | CSL_BootCfgClearResetMuxEvent (Uint8 coreIdx)
CSL_IDEF_INLINE void | CSL_BootCfgGetCOREPLLConfiguration (Uint32 *corePLLConfig0, Uint32 *corePLLConfig1)
CSL_IDEF_INLINE void | CSL_BootCfgSetCOREPLLConfiguration (Uint32 corePLLConfig0, Uint32 corePLLConfig1)
CSL_IDEF_INLINE void | CSL_BootCfgGetDDR3PLLConfiguration (Uint32 *ddr3PLLConfig0, Uint32 *ddr3PLLConfig1)
CSL_IDEF_INLINE void | CSL_BootCfgSetDDR3PLLConfiguration (Uint32 ddr3PLLConfig0, Uint32 ddr3PLLConfig1)
CSL_IDEF_INLINE void | CSL_BootCfgGetPAPLLConfiguration (Uint32 *paPLLConfig0, Uint32 *paPLLConfig1)
CSL_IDEF_INLINE void | CSL_BootCfgSetPAPLLConfiguration (Uint32 paPLLConfig0, Uint32 paPLLConfig1)
CSL_IDEF_INLINE void | CSL_BootCfgGetSGMIIConfigPLL (Uint16 *configPLL)
CSL_IDEF_INLINE void | CSL_BootCfgSetSGMIIConfigPLL (Uint16 configPLL)
CSL_IDEF_INLINE void | CSL_BootCfgGetSGMIIRxConfig (Uint8 index, Uint32 *rxConfig)
CSL_IDEF_INLINE void | CSL_BootCfgSetSGMIIRxConfig (Uint8 index, Uint32 rxConfig)
CSL_IDEF_INLINE void | CSL_BootCfgGetSGMIITxConfig (Uint8 index, Uint32 *txConfig)
CSL_IDEF_INLINE void | CSL_BootCfgSetSGMIITxConfig (Uint8 index, Uint32 txConfig)
CSL_IDEF_INLINE void | CSL_BootCfgGetSGMIIReserved (Uint32 *rsvdInfo)
CSL_IDEF_INLINE void | CSL_BootCfgSetSGMIIReserved (Uint32 rsvdInfo)
CSL_IDEF_INLINE void | CSL_BootCfgGetPCIEConfigPLL (Uint16 *config)
CSL_IDEF_INLINE void | CSL_BootCfgSetPCIEMode (Uint8 pcieMode)
CSL_IDEF_INLINE void | CSL_BootCfgGetPCIEPLLLock (Uint16 *lock)
CSL_IDEF_INLINE void | CSL_BootCfgSetPCIEConfigPLL (Uint16 config)
CSL_IDEF_INLINE void | CSL_BootCfgGetSRIOSERDESConfigPLL (Uint16 *config)
CSL_IDEF_INLINE void | CSL_BootCfgSetSRIOSERDESConfigPLL (Uint16 config)
CSL_IDEF_INLINE void | CSL_BootCfgGetPCIEReserved (Uint8 *rsvdInfo)
CSL_IDEF_INLINE void | CSL_BootCfgSetPCIEReserved (Uint8 rsvdInfo)
CSL_IDEF_INLINE void | CSL_BootCfgGetSRIOSERDESRxConfig (Uint8 index, Uint32 *config)
CSL_IDEF_INLINE void | CSL_BootCfgSetSRIOSERDESRxConfig (Uint8 index, Uint32 config)
CSL_IDEF_INLINE void | CSL_BootCfgGetSRIOSERDESTxConfig (Uint8 index, Uint32 *config)
CSL_IDEF_INLINE void | CSL_BootCfgSetSRIOSERDESTxConfig (Uint8 index, Uint32 config)
CSL_IDEF_INLINE void | CSL_BootCfgGetSRIOSERDESReserved (Uint32 *rsvdInfo)
CSL_IDEF_INLINE void | CSL_BootCfgSetSRIOSERDESReserved (Uint32 rsvdInfo)
CSL_IDEF_INLINE void | CSL_BootCfgGetLEDPassDoneStatus (Uint8 coreIdx, Uint8 *pass, Uint8 *done, Uint8 *idle, Uint8 *waitLoop)
CSL_IDEF_INLINE void | CSL_BootCfgSetLEDPassDoneStatus (Uint8 coreIdx, Uint8 pass, Uint8 done, Uint8 idle, Uint8 waitLoop)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsLEDPLLLocked (void)
CSL_IDEF_INLINE void | CSL_BootCfgLockLEDPLL (void)
CSL_IDEF_INLINE void | CSL_BootCfgUnlockLEDPLL (void)
CSL_IDEF_INLINE void | CSL_BootCfgGetLEDChipPassDoneStatus (Uint8 *pass, Uint8 *done)
CSL_IDEF_INLINE void | CSL_BootCfgSetLEDChipPassDoneStatus (Uint8 pass, Uint8 done)
CSL_IDEF_INLINE void | CSL_BootCfgGetDeviceSecureControl (Uint8 *vusrSecEnStatus, Uint8 *pbistSecEnStatus)
CSL_IDEF_INLINE void | CSL_BootCfgSetDeviceSecureControl (Uint8 vusrSecEnStatus, Uint8 pbistSecEnStatus)
CSL_IDEF_INLINE void | CSL_BootCfgGetROMChecksum (Uint32 *romLSBChecksum, Uint32 *romMSBChecksum)
CSL_IDEF_INLINE void | CSL_BootCfgGetCorePLLObservationClockControl (Uint8 *selection, Uint8 *enable)
CSL_IDEF_INLINE void | CSL_BootCfgSetCorePLLObservationClockControl (Uint8 selection, Uint8 enable)
CSL_IDEF_INLINE void | CSL_BootCfgGetDDR3PLLObservationClockControl (Uint8 *selection, Uint8 *enable)
CSL_IDEF_INLINE void | CSL_BootCfgSetDDR3PLLObservationClockControl (Uint8 selection, Uint8 enable)
CSL_IDEF_INLINE void | CSL_BootCfgGetPAPLLObservationClockControl (Uint8 *selection, Uint8 *enable)
CSL_IDEF_INLINE void | CSL_BootCfgSetPAPLLObservationClockControl (Uint8 selection, Uint8 enable)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsPSCEMIF4FResetEnabled (void)
CSL_IDEF_INLINE void | CSL_BootCfgEnablePSCEMIF4FReset (void)
CSL_IDEF_INLINE void | CSL_BootCfgDisablePSCEMIF4FReset (void)
CSL_IDEF_INLINE void | CSL_BootCfgGetVUSRConfigPLL (Uint16 *config)
CSL_IDEF_INLINE void | CSL_BootCfgSetVUSRConfigPLL (Uint16 config)
CSL_IDEF_INLINE void | CSL_BootCfgGetVUSRRxConfig (Uint8 index, Uint32 *config)
CSL_IDEF_INLINE void | CSL_BootCfgSetVUSRRxConfig (Uint8 index, Uint32 config)
CSL_IDEF_INLINE void | CSL_BootCfgGetVUSRTxConfig (Uint8 index, Uint32 *config)
CSL_IDEF_INLINE void | CSL_BootCfgSetVUSRTxConfig (Uint8 index, Uint32 config)
CSL_IDEF_INLINE void | CSL_BootCfgGetVUSRReserved (Uint32 *rsvdInfo)
CSL_IDEF_INLINE void | CSL_BootCfgSetVUSRReserved (Uint32 rsvdInfo)
CSL_IDEF_INLINE void | CSL_BootCfgGetQMPriority (Uint8 *qmprio)
CSL_IDEF_INLINE void | CSL_BootCfgSetQMPriority (Uint8 qmprio)
CSL_IDEF_INLINE void | CSL_BootCfgGetGEML2ReadLatency (Uint8 *latency)
CSL_IDEF_INLINE void | CSL_BootCfgSetGEML2ReadLatency (Uint8 latency)
CSL_IDEF_INLINE void | CSL_BootCfgGetGEML2AccessLatency (Uint8 *latency)
CSL_IDEF_INLINE void | CSL_BootCfgSetGEML2AccessLatency (Uint8 latency)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsDDR3PSCLockEnabled (void)
CSL_IDEF_INLINE void | CSL_BootCfgEnableDDR3PSCLock (void)
CSL_IDEF_INLINE void | CSL_BootCfgDisableDDR3PSCLock (void)
CSL_IDEF_INLINE Bool | CSL_BootCfgIsMSMCParityResetBlocked (void)
CSL_IDEF_INLINE void | CSL_BootCfgBlockMSMCParityReset (void)
CSL_IDEF_INLINE void | CSL_BootCfgUnblockMSMCParityReset (void)
CSL_IDEF_INLINE void | CSL_BootCfgGetDDRConfig (Uint8 regNum, Uint32 *ddr3Config)
CSL_IDEF_INLINE void | CSL_BootCfgSetDDRConfig (Uint8 regNum, Uint32 ddr3Config)

## Detailed Description

This is the Boot Configuration Auxilary Header File which exposes the various CSL Functional Layer API's to configure the BOOTCFG Module.

  ============================================================================
  (C) Copyright 2008, 2009, Texas Instruments, Inc.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.

Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.

Neither the name of Texas Instruments Incorporated nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Copyright 2012, Texas Instruments Incorporated