# Clock Mode
[TSIP Enumerated Data Types]

Clock Redundancy selection source. More...

## Enumerations
enum | CSL_TsipClkd { CSL_TSIP_CLKD_REDUN = 0, CSL_TSIP_CLKD_DUAL = 1 }

## Detailed Description

Clock Redundancy selection source.

Use this symbol to set the CLKD for redundancy clock selection

## Enumeration Type Documentation

enum CSL_TsipClkd

Enumerator:

  CSL_TSIP_CLKD_REDUN | Redundant Clock Mode
  CSL_TSIP_CLKD_DUAL | Dual Clock Mode

Copyright 2012, Texas Instruments Incorporated