# CSL_CPSW_3GF_ALE_OUIADDR_ENTRY Struct Reference
[CPSW_3GF Data Structures]

Holds the ALE OUI Unicast Address Table entry configuration. More...

`#include <csl_cpsw_3gf.h>`

## Data Fields
Uint8 | ouiAddress [3]
CSL_CPSW_3GF_ALE_UCASTTYPE | ucastType

## Detailed Description

Holds the ALE OUI Unicast Address Table entry configuration.

## Field Documentation

Uint8 CSL_CPSW_3GF_ALE_OUIADDR_ENTRY::ouiAddress[3]

OUI Unicast address

CSL_CPSW_3GF_ALE_UCASTTYPE CSL_CPSW_3GF_ALE_OUIADDR_ENTRY::ucastType

Unicast type

The documentation for this struct was generated from the following file:

- csl_cpsw_3gf.h

Copyright 2012, Texas Instruments Incorporated