# CSL_CPSW_3GF_ALE_VLANMCASTADDR_ENTRY Struct Reference
[CPSW_3GF Data Structures]

Holds the ALE VLAN/Multicast Address Table entry configuration. More...

`#include <csl_cpsw_3gf.h>`

## Data Fields
Uint8 | macAddress [6]
Uint32 | vlanId
Uint32 | mcastFwdState
Uint32 | superEnable
Uint32 | portMask

## Detailed Description

Holds the ALE VLAN/Multicast Address Table entry configuration.

## Field Documentation

Uint8 CSL_CPSW_3GF_ALE_VLANMCASTADDR_ENTRY::macAddress[6]

Multicast address

Uint32 CSL_CPSW_3GF_ALE_VLANMCASTADDR_ENTRY::mcastFwdState

Multicast forward state

Uint32 CSL_CPSW_3GF_ALE_VLANMCASTADDR_ENTRY::portMask

Port Mask.

Uint32 CSL_CPSW_3GF_ALE_VLANMCASTADDR_ENTRY::superEnable

Supervisory bit enable?

Uint32 CSL_CPSW_3GF_ALE_VLANMCASTADDR_ENTRY::vlanId

VLAN Id

The documentation for this struct was generated from the following file:

- csl_cpsw_3gf.h

Copyright 2012, Texas Instruments Incorporated