# CSL_BWMNGMT_CPUARB_SETUP Struct Reference
[BWMNGMT Data Structures]

CSL_BWMNGMT_CPUARB_SETUP has all the fields required to configure the CPU Arbitration Control Register of BWMNGMT for any given memory control block (L1D/L2/EMC). More...

`#include <csl_bwmngmt.h>`

## Data Fields
Uint32 | priority
Uint32 | maxWait

## Detailed Description

CSL_BWMNGMT_CPUARB_SETUP has all the fields required to configure the CPU Arbitration Control Register of BWMNGMT for any given memory control block (L1D/L2/EMC).

## Field Documentation

Uint32 CSL_BWMNGMT_CPUARB_SETUP::maxWait

CPU - Requestor Arbitration Settings - MAXWAIT

Uint32 CSL_BWMNGMT_CPUARB_SETUP::priority

CPU - Requestor Arbitration Settings - PRI

The documentation for this struct was generated from the following file:

- csl_bwmngmt.h

Copyright 2012, Texas Instruments Incorporated