# Data Rate
[TSIP Enumerated Data Types]

Data Rate supported on TSIP. More...

## Enumerations
enum | CSL_TsipDataRate { CSL_TSIP_DATARATE_8M = 0, CSL_TSIP_DATARATE_16M = 1, CSL_TSIP_DATARATE_32M = 2 }

## Detailed Description

Data Rate supported on TSIP.

Use this symbol for setting Data rate

## Enumeration Type Documentation

enum CSL_TsipDataRate

Enumerator:

  CSL_TSIP_DATARATE_8M | Data rate is 8 Mbps
  CSL_TSIP_DATARATE_16M | Data rate is 16 Mbps
  CSL_TSIP_DATARATE_32M | Data rate is 32 Mbps

Copyright 2012, Texas Instruments Incorporated