# CSL_Edma3QueStat Struct Reference
[EDMA3 Data Structures]

Edma Controller Que Status. More...

`#include <csl_edma3.h>`

## Data Fields
CSL_Edma3Que | que
Bool | exceed
Uint8 | waterMark
Uint8 | numVal
Uint8 | startPtr

## Detailed Description

Edma Controller Que Status.

An object of this type is allocated by the user and its address is passed as a parameter to the CSL_edma3GetQueStatus() /CSL_edma3GetHwStatus().

## Field Documentation

Bool CSL_Edma3QueStat::exceed

Output field: The number of valid entries in a queue has exceeded the threshold specified in QWMTHRA has been exceeded

Uint8 CSL_Edma3QueStat::numVal

Output field: Number of valid entries in Que N

CSL_Edma3Que CSL_Edma3QueStat::que

Input field: Event Que. This needs to be specified by the user before invocation of the above API

Uint8 CSL_Edma3QueStat::startPtr

Output field: Start pointer/Head of the queue

Uint8 CSL_Edma3QueStat::waterMark

Output field: The most entries that have been in Que since reset/last time the watermark was cleared

The documentation for this struct was generated from the following file:

- csl_edma3.h

Copyright 2012, Texas Instruments Incorporated