# CSL_CPSW_3GF_TSCNTL Struct Reference
[CPSW_3GF Data Structures]

Holds Port Time Sync Control register contents. More...

`#include <csl_cpsw_3gf.h>`

## Data Fields
Uint32 | tsRxEnable
Uint32 | tsRxVlanLType1Enable
Uint32 | tsRxVlanLType2Enable
Uint32 | tsTxEnable
Uint32 | tsTxVlanLType1Enable
Uint32 | tsTxVlanLType2Enable
Uint32 | txMsgTypeEnable

## Detailed Description

Holds Port Time Sync Control register contents.

## Field Documentation

Uint32 CSL_CPSW_3GF_TSCNTL::tsRxEnable

Port Time sync receive enable bit

Uint32 CSL_CPSW_3GF_TSCNTL::tsRxVlanLType1Enable

Port Time sync receive VLAN LTYPE 1 enable bit

Uint32 CSL_CPSW_3GF_TSCNTL::tsRxVlanLType2Enable

Port Time sync receive VLAN LTYPE 2 enable bit

Uint32 CSL_CPSW_3GF_TSCNTL::tsTxEnable

Port Time sync transmit enable bit

Uint32 CSL_CPSW_3GF_TSCNTL::tsTxVlanLType1Enable

Port Time sync transmit VLAN LTYPE 1 enable bit

Uint32 CSL_CPSW_3GF_TSCNTL::tsTxVlanLType2Enable

Port Time sync transmit VLAN LTYPE 2 enable bit

Uint32 CSL_CPSW_3GF_TSCNTL::txMsgTypeEnable

Port Time sync message type enable bit

The documentation for this struct was generated from the following file:

- csl_cpsw_3gf.h

Copyright 2012, Texas Instruments Incorporated