# Output Enanble Delay
[TSIP Enumerated Data Types]

TSIP Output Enanble Delay. More...

## Enumerations
enum | CSL_TsipDlyCtrl { CSL_TSIP_DLY_CTRL_DISABLE = 0, CSL_TSIP_DLY_CTRL_ENABLE = 1 }

## Detailed Description

TSIP Output Enanble Delay.

Use this symbol to represent Output Enanble Delay This symbol is used on both RCV and XMT

## Enumeration Type Documentation

enum CSL_TsipDlyCtrl

Enumerator:

  CSL_TSIP_DLY_CTRL_DISABLE | No Added Delay
  CSL_TSIP_DLY_CTRL_ENABLE | Active High

Copyright 2012, Texas Instruments Incorporated