# CSL_MEMPROT_MPFSR Struct Reference
[MEMPROT Data Structures]

This will be used to query the memory fault status. More...

`#include <csl_memprot.h>`

## Data Fields
Uint32 | fid:7
Uint32 | local:1
Uint32 | ns:1
Uint32 | sr:1
Uint32 | sw:1
Uint32 | sx:1
Uint32 | ur:1
Uint32 | uw:1
Uint32 | ux:1

## Detailed Description

This will be used to query the memory fault status.

## Field Documentation

Uint32 CSL_MEMPROT_MPFSR::fid

Faulted ID

Uint32 CSL_MEMPROT_MPFSR::local

Local Access ?

Uint32 CSL_MEMPROT_MPFSR::ns

When set, indicates a Non-secure access

Uint32 CSL_MEMPROT_MPFSR::sr

When set, indicates a Supervisor Read Request

Uint32 CSL_MEMPROT_MPFSR::sw

When set, indicates a Supervisor Write Request

Uint32 CSL_MEMPROT_MPFSR::sx

When set, indicates a Supervisor program fetch Request

Uint32 CSL_MEMPROT_MPFSR::ur

When set, indicates a User Read Request

Uint32 CSL_MEMPROT_MPFSR::uw

When set, indicates a User Write Request

Uint32 CSL_MEMPROT_MPFSR::ux

When set, indicates a User program fetch Request

The documentation for this struct was generated from the following file:

- csl_memprot.h

Copyright 2012, Texas Instruments Incorporated