# TIMER Data Structures
[TIMER]

## Data Structures
struct | CSL_TmrHwSetup
| Hardware setup structure. More...
struct | CSL_TmrConfig
| Config-structure Used to configure the GP timer using CSL_tmrHwSetupRaw(). More...
struct | CSL_TmrContext
| Module specific context information. Present implementation of GP timer CSL doesn't have any context information. More...
struct | CSL_TmrParam
| Module specific parameters. Present implementation of GP timer CSL doesn't have any module specific parameters. More...
struct | CSL_TmrBaseAddress
| This structure contains the base-address information for the peripheral instance. More...
struct | CSL_TmrObj
| Watchdog timer object structure. More...
## Typedefs
typedef CSL_TmrObj * | CSL_TmrHandle
| This data type is used to return the handle to the CSL of the GP timer.

Copyright 2012, Texas Instruments Incorporated