# Emulation mode setting
[TSIP Enumerated Data Types]

Emulation mode setting. More...

## Enumerations
enum | CSL_TsipEmu { CSL_TSIP_EMU_STOP = 0, CSL_TSIP_EMU_TX_STOP = 1, CSL_TSIP_EMU_FREERUN = 2 }

## Detailed Description

Emulation mode setting.

Use this symbol to set the Emulation Mode

## Enumeration Type Documentation

enum CSL_TsipEmu

Enumerator:

  CSL_TSIP_EMU_STOP | Emulation mode stop
  CSL_TSIP_EMU_TX_STOP | Emulation mode TX stop
  CSL_TSIP_EMU_FREERUN | Emulation free run mode

Copyright 2012, Texas Instruments Incorporated