# CSL_Edma3CmdQrae Struct Reference
[EDMA3 Data Structures]

Edma Control/Query Command Structure for querying qdma region access enable attributes. More...

`#include <csl_edma3.h>`

## Data Fields
Int | region
CSL_BitMask32 | qrae

## Detailed Description

Edma Control/Query Command Structure for querying qdma region access enable attributes.

An object of this type is allocated by the user and its address is passed as a parameter to the CSL_edma3GetHwStatus/CSL_edma3HwControl with the relevant command.

## Field Documentation

CSL_BitMask32 CSL_Edma3CmdQrae::qrae

this needs to be filled by the user in case of issuing a COMMAND or it will be filled in by the CSL when used with a QUERY

Int CSL_Edma3CmdQrae::region

this field needs to be initialized by the user before issuing the query/command

The documentation for this struct was generated from the following file:

- csl_edma3.h

Copyright 2012, Texas Instruments Incorporated