# CSL_MDIO_USERPHYSEL Struct Reference
[MDIO Data Structures]

Holds the MDIO User Phy Select Register contents. More...

`#include <csl_mdio.h>`

## Data Fields
Uint16 | linkSel
Uint32 | bLinkIntEnable
Uint32 | phyAddr

## Detailed Description

Holds the MDIO User Phy Select Register contents.

## Field Documentation

Uint32 CSL_MDIO_USERPHYSEL::bLinkIntEnable

Link Status Change Interrupt Enable bit

Uint16 CSL_MDIO_USERPHYSEL::linkSel

Link Status determination select bit. Always reads '0'

Uint32 CSL_MDIO_USERPHYSEL::phyAddr

Phy Device Address

The documentation for this struct was generated from the following file:

- csl_mdio.h

Copyright 2012, Texas Instruments Incorporated