# CSL_CPSW_3GF_PORTSTAT Struct Reference
[CPSW_3GF Data Structures]

Holds Port Statistics Enable register contents. More...

`#include <csl_cpsw_3gf.h>`

## Data Fields
Uint32 | p0AStatEnable
Uint32 | p0BStatEnable
Uint32 | p1StatEnable
Uint32 | p2StatEnable

## Detailed Description

Holds Port Statistics Enable register contents.

## Field Documentation

Uint32 CSL_CPSW_3GF_PORTSTAT::p0AStatEnable

Port 0 Statistics A Enable bit

Uint32 CSL_CPSW_3GF_PORTSTAT::p0BStatEnable

Port 0 Statistics B Enable bit

Uint32 CSL_CPSW_3GF_PORTSTAT::p1StatEnable

Port 1 Statistics Enable bit

Uint32 CSL_CPSW_3GF_PORTSTAT::p2StatEnable

Port 2 Statistics Enable bit

The documentation for this struct was generated from the following file:

- csl_cpsw_3gf.h

Copyright 2012, Texas Instruments Incorporated