# CSL_MEMPROT_MPLKSTAT Struct Reference
[MEMPROT Data Structures]

This will be used to lock/unlock/reset a memory region. More...

`#include <csl_memprot.h>`

## Data Fields
Uint32 | nsl:1
Uint32 | lk:1

## Detailed Description

This will be used to lock/unlock/reset a memory region.

## Field Documentation

Uint32 CSL_MEMPROT_MPLKSTAT::lk

Indicates the Lock Status; 1 indicates Locked, 0 means disengaged.

Uint32 CSL_MEMPROT_MPLKSTAT::nsl

Indicates whether Emulation and Non secure may manipulate the lock hardware.

The documentation for this struct was generated from the following file:

- csl_memprot.h

Copyright 2012, Texas Instruments Incorporated