# CSL_CPSW_3GF_CONTROL Struct Reference
[CPSW_3GF Data Structures]

Holds CPSW control register contents. More...

`#include <csl_cpsw_3gf.h>`

## Data Fields
Uint32 | fifoLb
Uint32 | vlanAware
Uint32 | p0Enable
Uint32 | p0PassPriTag
Uint32 | p1PassPriTag
Uint32 | p2PassPriTag

## Detailed Description

Holds CPSW control register contents.

## Field Documentation

Uint32 CSL_CPSW_3GF_CONTROL::fifoLb

FIFO loopback mode

Uint32 CSL_CPSW_3GF_CONTROL::p0Enable

Port 0 Enable

Uint32 CSL_CPSW_3GF_CONTROL::p0PassPriTag

Port 0 Pass Priority Tagged

Uint32 CSL_CPSW_3GF_CONTROL::p1PassPriTag

Port 1 Pass Priority Tagged

Uint32 CSL_CPSW_3GF_CONTROL::p2PassPriTag

Port 2 Pass Priority Tagged

Uint32 CSL_CPSW_3GF_CONTROL::vlanAware

Vlan aware mode

The documentation for this struct was generated from the following file:

- csl_cpsw_3gf.h

Copyright 2012, Texas Instruments Incorporated