# csl_srioAux.h File Reference

This is the SRIO Auxilary Header File which exposes the various CSL Functional Layer API's to configure the SRIO Module. More...

`#include <ti/csl/soc.h>`
`#include <ti/csl/csl_srio.h>`

## Functions
CSL_IDEF_INLINE void | CSL_SRIO_GetPID (CSL_SrioHandle hSrio, Uint32 *pid)
CSL_IDEF_INLINE void | CSL_SRIO_EnablePeripheral (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_DisablePeripheral (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_SetMAUSwappingMode (CSL_SrioHandle hSrio, Uint8 mode)
CSL_IDEF_INLINE void | CSL_SRIO_GetMAUSwappingMode (CSL_SrioHandle hSrio, Uint8 *mode)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUSwappingMode (CSL_SrioHandle hSrio, Uint8 mode)
CSL_IDEF_INLINE void | CSL_SRIO_GetLSUSwappingMode (CSL_SrioHandle hSrio, Uint8 *mode)
CSL_IDEF_INLINE void | CSL_SRIO_EnablePromiscuous (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_DisablePromiscuous (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE Bool | CSL_SRIO_IsPromiscuous (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_SetAMUSwappingMode (CSL_SrioHandle hSrio, Uint8 mode)
CSL_IDEF_INLINE void | CSL_SRIO_GetAMUSwappingMode (CSL_SrioHandle hSrio, Uint8 *mode)
CSL_IDEF_INLINE void | CSL_SRIO_SetBootComplete (CSL_SrioHandle hSrio, Uint8 bootCompleteFlag)
CSL_IDEF_INLINE void | CSL_SRIO_GetBootComplete (CSL_SrioHandle hSrio, Uint8 *bootCompleteFlag)
CSL_IDEF_INLINE void | CSL_SRIO_SetTXURXUSwappingMode (CSL_SrioHandle hSrio, Uint8 mode)
CSL_IDEF_INLINE void | CSL_SRIO_GetTXURXUSwappingMode (CSL_SrioHandle hSrio, Uint8 *mode)
CSL_IDEF_INLINE void | CSL_SRIO_EnableAutomaticPriorityPromotion (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_DisableAutomaticPriorityPromotion (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE Bool | CSL_SRIO_IsAutomaticPriorityPromotionEnabled (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_SetTxCreditThreshold (CSL_SrioHandle hSrio, Uint8 priority, Uint8 credit)
CSL_IDEF_INLINE void | CSL_SRIO_GetTxCreditThreshold (CSL_SrioHandle hSrio, Uint8 priority, Uint8 *credit)
CSL_IDEF_INLINE void | CSL_SRIO_SetTransactionPriority (CSL_SrioHandle hSrio, Uint8 priority)
CSL_IDEF_INLINE void | CSL_SRIO_GetTransactionPriority (CSL_SrioHandle hSrio, Uint8 *priority)
CSL_IDEF_INLINE void | CSL_SRIO_SetPrescalarSelect (CSL_SrioHandle hSrio, Uint8 prescalarSelect)
CSL_IDEF_INLINE void | CSL_SRIO_GetPrescalarSelect (CSL_SrioHandle hSrio, Uint8 *prescalarSelect)
CSL_IDEF_INLINE void | CSL_SRIO_SetResponseCRF (CSL_SrioHandle hSrio, Uint8 value)
CSL_IDEF_INLINE void | CSL_SRIO_GetResponseCRF (CSL_SrioHandle hSrio, Uint8 *value)
CSL_IDEF_INLINE void | CSL_SRIO_SetRXUWatermark (CSL_SrioHandle hSrio, Uint8 value)
CSL_IDEF_INLINE void | CSL_SRIO_GetRXUWatermark (CSL_SrioHandle hSrio, Uint8 *value)
CSL_IDEF_INLINE void | CSL_SRIO_SetSysClkSel (CSL_SrioHandle hSrio, Uint8 value)
CSL_IDEF_INLINE void | CSL_SRIO_GetSysClkSel (CSL_SrioHandle hSrio, Uint8 *value)
CSL_IDEF_INLINE void | CSL_SRIO_SetLoopbackMode (CSL_SrioHandle hSrio, Uint8 portNum)
CSL_IDEF_INLINE void | CSL_SRIO_SetNormalMode (CSL_SrioHandle hSrio, Uint8 portNum)
CSL_IDEF_INLINE Bool | CSL_SRIO_IsLoopbackMode (CSL_SrioHandle hSrio, Uint8 portNum)
CSL_IDEF_INLINE void | CSL_SRIO_EnableCOS (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_DisableCOS (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE Bool | CSL_SRIO_IsCOSEnabled (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_GlobalEnable (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_GlobalDisable (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE Bool | CSL_SRIO_IsSRIOEnabled (CSL_SrioHandle hSrio)
CSL_IDEF_INLINE void | CSL_SRIO_EnableBlock (CSL_SrioHandle hSrio, Uint16 blockNumber)
CSL_IDEF_INLINE void | CSL_SRIO_DisableBlock (CSL_SrioHandle hSrio, Uint16 blockNumber)
CSL_IDEF_INLINE Bool | CSL_SRIO_IsSRIOBlockEnabled (CSL_SrioHandle hSrio, Uint16 blockNumber)
CSL_IDEF_INLINE void | CSL_SRIO_SetDeviceID (CSL_SrioHandle hSrio, Uint8 index, Uint8 NodeId8bit, Uint16 NodeId16bit)
CSL_IDEF_INLINE void | CSL_SRIO_GetDeviceID (CSL_SrioHandle hSrio, Uint8 index, Uint8 *NodeId8bit, Uint16 *NodeId16bit)
CSL_IDEF_INLINE void | CSL_SRIO_SetPacketForwarding (CSL_SrioHandle hSrio, Uint8 index, Uint16 low16bitDeviceID, Uint16 up16bitDeviceID, Uint8 low8bitDeviceID, Uint8 up8bitDeviceID, Uint8 outPort)
CSL_IDEF_INLINE void | CSL_SRIO_GetPacketForwarding (CSL_SrioHandle hSrio, Uint8 index, Uint16 *low16bitDeviceID, Uint16 *up16bitDeviceID, Uint8 *low8bitDeviceID, Uint8 *up8bitDeviceID, Uint8 *outPort)
CSL_IDEF_INLINE void | CSL_SRIO_GetDoorbellPendingInterrupt (CSL_SrioHandle hSrio, Uint8 port, Uint16 *doorbellStatus)
CSL_IDEF_INLINE void | CSL_SRIO_ClearDoorbellPendingInterrupt (CSL_SrioHandle hSrio, Uint8 port, Uint16 doorbellInterrupt)
CSL_IDEF_INLINE void | CSL_SRIO_GetLSUPendingInterrupt (CSL_SrioHandle hSrio, Uint32 *lsuStatus1, Uint32 *lsuStatus2)
CSL_IDEF_INLINE void | CSL_SRIO_ClearLSUPendingInterrupt (CSL_SrioHandle hSrio, Uint32 lsuInterrupt1, Uint32 lsuInterrupt2)
CSL_IDEF_INLINE void | CSL_SRIO_ClearLSU0PendingInterrupt (CSL_SrioHandle hSrio, Uint32 lsuInterrupt)
CSL_IDEF_INLINE void | CSL_SRIO_GetErrorPendingInterrupt (CSL_SrioHandle hSrio, Uint32 *errStatus)
CSL_IDEF_INLINE void | CSL_SRIO_ClearErrorPendingInterrupt (CSL_SrioHandle hSrio, Uint32 errStatus)
CSL_IDEF_INLINE void | CSL_SRIO_GetAMUPendingInterrupt (CSL_SrioHandle hSrio, Uint16 *amuIntrStatus)
CSL_IDEF_INLINE void | CSL_SRIO_ClearAMUPendingInterrupt (CSL_SrioHandle hSrio, Uint16 amuIntrStatus)
CSL_IDEF_INLINE void | CSL_SRIO_RouteDoorbellInterrupts (CSL_SrioHandle hSrio, Uint8 regNum, Uint8 doorBellBit, Uint8 destination)
CSL_IDEF_INLINE void | CSL_SRIO_RouteLSUInterrupts (CSL_SrioHandle hSrio, Uint8 lsuIntrReq, Uint8 destination)
CSL_IDEF_INLINE void | CSL_SRIO_RouteErrorInterrupts (CSL_SrioHandle hSrio, Uint8 errIntrReq, Uint8 destination)
CSL_IDEF_INLINE void | CSL_SRIO_RouteAMUInterrupts (CSL_SrioHandle hSrio, Uint8 amuIntr, Uint8 destination)
CSL_IDEF_INLINE void | CSL_SRIO_GetDoorbellRoute (CSL_SrioHandle hSrio, Uint8 *routeInfo)
CSL_IDEF_INLINE void | CSL_SRIO_SetDoorbellRoute (CSL_SrioHandle hSrio, Uint8 routeInfo)
CSL_IDEF_INLINE void | CSL_SRIO_GetInterruptStatusDecode (CSL_SrioHandle hSrio, Uint8 intrDst, Uint32 *status)
CSL_IDEF_INLINE void | CSL_SRIO_EnableInterruptPacing (CSL_SrioHandle hSrio, Uint8 destination)
CSL_IDEF_INLINE void | CSL_SRIO_DisableInterruptPacing (CSL_SrioHandle hSrio, Uint8 destination)
CSL_IDEF_INLINE void | CSL_SRIO_SetInterruptPacing (CSL_SrioHandle hSrio, Uint8 destination, Uint32 rate)
CSL_IDEF_INLINE void | CSL_SRIO_GetInterruptRate (CSL_SrioHandle hSrio, Uint8 destination, Uint32 *rate)
CSL_IDEF_INLINE void | CSL_SRIO_SetType11PSInfo (Uint32 psInfo[2], Uint16 dstId, Uint16 srcId, Uint8 mbox, Uint8 letter, Uint8 tt, Uint8 ssize, Uint8 retryCount)
CSL_IDEF_INLINE void | CSL_SRIO_ExtractType11PSInfo (Uint32 psInfo[2], Uint16 *dstId, Uint16 *srcId, Uint8 *mbox, Uint8 *letter, Uint8 *tt, Uint8 *pri, Uint8 *cc)
CSL_IDEF_INLINE void | CSL_SRIO_MapMessageToQueue (CSL_SrioHandle hSrio, Uint8 index, SRIO_MESSAGE *ptrMessage, Uint16 queueId)
CSL_IDEF_INLINE void | CSL_SRIO_GetMessageToQueueMapping (CSL_SrioHandle hSrio, Uint8 index, SRIO_MESSAGE *ptrMessage, Uint16 *queueId)
CSL_IDEF_INLINE void | CSL_SRIO_SetType9PSInfo (Uint32 psInfo[2], Uint16 dstId, Uint16 srcId, Uint8 cos, Uint8 cosMask, Uint8 tt, Uint16 streamId)
CSL_IDEF_INLINE void | CSL_SRIO_ExtractType9PSInfo (Uint32 psInfo[2], Uint16 *dstId, Uint16 *srcId, Uint8 *cos, Uint8 *cc, Uint8 *tt, Uint8 *pri, Uint16 *streamId)
CSL_IDEF_INLINE void | CSL_SRIO_MapType9MessageToQueue (CSL_SrioHandle hSrio, Uint8 index, SRIO_TYPE9_MESSAGE *ptrMessage, Uint16 queueId)
CSL_IDEF_INLINE void | CSL_SRIO_GetType9MessageToQueueMapping (CSL_SrioHandle hSrio, Uint8 index, SRIO_TYPE9_MESSAGE *ptrMessage, Uint16 *queueId)
CSL_IDEF_INLINE void | CSL_SRIO_MapAMUPrivIdToSourceId (CSL_SrioHandle hSrio, Uint8 privId, Uint8 srcId)
CSL_IDEF_INLINE void | CSL_SRIO_GetAMUPrivIdToSourceIdMapping (CSL_SrioHandle hSrio, Uint8 privId, Uint8 *srcId)
CSL_IDEF_INLINE void | CSL_SRIO_MapVBUSPriorityToRIO (CSL_SrioHandle hSrio, Uint8 vbusPriority, Uint8 priority)
CSL_IDEF_INLINE void | CSL_SRIO_GetVBUSPriorityToRIOMapping (CSL_SrioHandle hSrio, Uint8 vbusPriority, Uint8 *priority)
CSL_IDEF_INLINE void | CSL_SRIO_GetAMUErrorCaptureInfo (CSL_SrioHandle hSrio, Uint32 *transAddress, Uint8 *privId, Uint8 *mstID, Uint16 *doorbellInfo)
CSL_IDEF_INLINE void | CSL_SRIO_SetAMUWindow (CSL_SrioHandle hSrio, Uint8 index, SRIO_AMU_WINDOW *amuWindow)
CSL_IDEF_INLINE void | CSL_SRIO_GetAMUWindow (CSL_SrioHandle hSrio, Uint8 index, SRIO_AMU_WINDOW *amuWindow)
CSL_IDEF_INLINE void | CSL_SRIO_SetAMUPane (CSL_SrioHandle hSrio, Uint8 index, SRIO_AMU_PANE *amuPane)
CSL_IDEF_INLINE void | CSL_SRIO_GetAMUPane (CSL_SrioHandle hSrio, Uint8 index, SRIO_AMU_PANE *amuPane)
CSL_IDEF_INLINE void | CSL_SRIO_SetAMUFlowMask (CSL_SrioHandle hSrio, Uint16 flowMask)
CSL_IDEF_INLINE void | CSL_SRIO_GetAMUFlowMask (CSL_SrioHandle hSrio, Uint16 *flowMask)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUTransfer (CSL_SrioHandle hSrio, Uint8 lsu, SRIO_LSU_TRANSFER *lsuTransfer)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUReg0 (CSL_SrioHandle hSrio, Uint8 lsu, Uint32 rapidIOMSB)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUReg1 (CSL_SrioHandle hSrio, Uint8 lsu, Uint32 rapidIOLSB)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUReg2 (CSL_SrioHandle hSrio, Uint8 lsu, Uint32 dspAddress)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUReg3 (CSL_SrioHandle hSrio, Uint8 lsu, Uint32 byteCount, Uint8 doorbellValid)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUReg4 (CSL_SrioHandle hSrio, Uint8 lsu, Uint16 dstId, Uint8 srcIdMap, Uint8 idSize, Uint8 outPortId, Uint8 priority, Uint8 xambs, Uint8 supGoodInt, Uint8 intRequest)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUReg5 (CSL_SrioHandle hSrio, Uint8 lsu, Uint8 ttype, Uint8 ftype, Uint8 hopCount, Uint16 doorbellInfo)
CSL_IDEF_INLINE Bool | CSL_SRIO_IsLSUFull (CSL_SrioHandle hSrio, Uint8 lsu)
CSL_IDEF_INLINE Bool | CSL_SRIO_IsLSUBusy (CSL_SrioHandle hSrio, Uint8 lsu)
CSL_IDEF_INLINE void | CSL_SRIO_GetLSUContextTransaction (CSL_SrioHandle hSrio, Uint8 lsu, Uint8 *context, Uint8 *transID)
CSL_IDEF_INLINE void | CSL_SRIO_CancelLSUTransaction (CSL_SrioHandle hSrio, Uint8 lsu, Uint8 privID)
CSL_IDEF_INLINE void | CSL_SRIO_RestartLSUTransaction (CSL_SrioHandle hSrio, Uint8 lsu)
CSL_IDEF_INLINE void | CSL_SRIO_FlushLSUTransaction (CSL_SrioHandle hSrio, Uint8 lsu, Uint8 srcIDMap)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUShadowRegs (CSL_SrioHandle hSrio, Uint32 shadowGrp0, Uint32 shadowGrp1)
CSL_IDEF_INLINE void | CSL_SRIO_GetLSUShadowRegs (CSL_SrioHandle hSrio, Uint8 index, Uint8 *count)
CSL_IDEF_INLINE void | CSL_SRIO_EnableSrcIDInterrupts (CSL_SrioHandle hSrio, Uint8 index)
CSL_IDEF_INLINE void | CSL_SRIO_DisableSrcIDInterrupts (CSL_SrioHandle hSrio, Uint8 index)
CSL_IDEF_INLINE void | CSL_SRIO_SetTimeoutCnt (CSL_SrioHandle hSrio, Uint8 timeoutCnt)
CSL_IDEF_INLINE void | CSL_SRIO_GetTimeoutCnt (CSL_SrioHandle hSrio, Uint8 *timeoutCnt)
CSL_IDEF_INLINE void | CSL_SRIO_GetLSUCompletionCode (CSL_SrioHandle hSrio, Uint8 lsu, Uint8 transID, Uint8 *compCode, Uint8 *contextBit)
CSL_IDEF_INLINE void | CSL_SRIO_SetLSUFlowMask (CSL_SrioHandle hSrio, Uint8 lsu, Uint16 flowMask)
CSL_IDEF_INLINE void | CSL_SRIO_GetLSUFlowMask (CSL_SrioHandle hSrio, Uint8 lsu, Uint16 *flowMask)
CSL_IDEF_INLINE void | CSL_SRIO_SetSupervisorPerms (CSL_SrioHandle hSrio, Uint16 supervisor16ID, Uint8 supervisor8ID)
CSL_IDEF_INLINE void | CSL_SRIO_GetSupervisorPerms (CSL_SrioHandle hSrio, Uint16 *supervisor16ID, Uint8 *supervisor8ID)
CSL_IDEF_INLINE void | CSL_SRIO_SetFlowControl (CSL_SrioHandle hSrio, Uint8 flowControlIdx, Uint8 tt, Uint16 dstID)
CSL_IDEF_INLINE void | CSL_SRIO_GetFlowControl (CSL_SrioHandle hSrio, Uint8 flowControlIdx, Uint8 *tt, Uint16 *dstID)
CSL_IDEF_INLINE void | CSL_SRIO_SetTxCPPIFlowMask (CSL_SrioHandle hSrio, Uint8 txCPPI, Uint16 flowMask)
CSL_IDEF_INLINE void | CSL_SRIO_GetTxCPPIFlowMask (CSL_SrioHandle hSrio, Uint8 txCPPI, Uint16 *flowMask)
CSL_IDEF_INLINE void | CSL_SRIO_SetTxQueueSchedInfo (CSL_SrioHandle hSrio, Uint8 txQueue, Uint8 portNum, Uint8 crf)
CSL_IDEF_INLINE void | CSL_SRIO_GetTxQueueSchedInfo (CSL_SrioHandle hSrio, Uint8 txQueue, Uint8 *portNum, Uint8 *priority, Uint8 *crf)
CSL_IDEF_INLINE void | CSL_SRIO_SetTxGarbageCollectionInfo (CSL_SrioHandle hSrio, Uint16 qidLength, Uint16 qidTimeout, Uint16 qidRetry, Uint16 qidTransErr, Uint16 qidProg, Uint16 qidSsize)
CSL_IDEF_INLINE void | CSL_SRIO_GetTxGarbageCollectionInfo (CSL_SrioHandle hSrio, Uint16 *qidLength, Uint16 *qidTimeout, Uint16 *qidRetry, Uint16 *qidTransErr, Uint16 *qidProg, Uint16 *qidSsize)
CSL_IDEF_INLINE void | CSL_SRIO_GetQMBaseAddress (CSL_SrioHandle hSrio, Uint8 qmIndex, Uint32 *qmBaseAddress)
CSL_IDEF_INLINE void | CSL_SRIO_SetQMBaseAddress (CSL_SrioHandle hSrio, Uint8 qmIndex, Uint32 qmBaseAddress)

## Detailed Description

This is the SRIO Auxilary Header File which exposes the various CSL Functional Layer API's to configure the SRIO Module.

  ============================================================================
  (C) Copyright 2008-2011, Texas Instruments, Inc.

Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.

Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.

Neither the name of Texas Instruments Incorporated nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

Copyright 2012, Texas Instruments Incorporated